IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView]"
File name: "0001"
Time stamp: "2021-12-14T20:57:18"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190808_0900(x64) - Exporter 19.2.20.24 - Alternate UI 19.2.20.24"
Application: "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)"

People and organizations
  Person "info@bimetica.com" of Organization (no name given)
  Owner history of Person "info@bimetica.com" of Organization (no name given) | application "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)" | change NOCHANGE | created 1639502555 (2021-12-14T17:22:35Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "## Street City, State Zip", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 2 elements
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Generic - 200mm" | object type "Basic Wall:Generic - 200mm:249" | names: "Basic Wall:Generic - 200mm:359791" | material: layers "Basic Wall:Generic - 200mm" ("Default Wall" 200.) | property sets: BaseQuantities, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCWINDOW | type IFCWINDOWSTYLE "1230x1480 mm - Practicable" | object type "1230x1480 mm - Practicable" | names: "2019_ES_Ventana_QSystems_Q67+_2-Hojas:1230x1480 mm - Practicable:361645" | material: materials ("Technoform Warm Edge", "Aluminio Anodizado, lacado") | property sets: Pset_WindowCommon, Pset_ManufacturerTypeInformation, BaseQuantities, Constraints, Dimensions, Identity Data

Types
  IFCWALLTYPE "Basic Wall:Generic - 200mm" | STANDARD | 1 occurrence | material: layers "Basic Wall:Generic - 200mm" ("Default Wall" 200.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWINDOWSTYLE "1230x1480 mm - Practicable" | 1 occurrence | material: materials ("Technoform Warm Edge", "Aluminio Anodizado, lacado") | property sets: 2019_ES_Ventana_QSystems_Q67+_2-Hojas:1230x1480 mm - Practicable:361645, Analysis Results, Analytical Properties, Construction, Data, Dimensions

Property sets
  BaseQuantities | quantities | on 1 object (1 IFCWALLSTANDARDCASE)
    GrossFootprintArea = 0.6 [SQUARE_METRE]
    GrossSideArea = 7.17960000000001 [SQUARE_METRE]
    GrossVolume = 1.43592 [CUBIC_METRE]
    Height = 3000. [MILLI METRE]
    Length = 3000. [MILLI METRE]
    Width = 200. [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCWINDOW)
    Area = 2.44709616574625 [SQUARE_METRE]
    Height = 1480. [MILLI METRE]
    Width = 1230. [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCOPENINGELEMENT)
    Depth = 200. [MILLI METRE]
    Height = 1230. [MILLI METRE]
    Width = 1480. [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: Level 1" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Wall Centerline" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 3000. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCWINDOW)
    Level = "Level: Level 1" (IFCLABEL)
    Sill Height = 700. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 7.17960000000001 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3000. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 1.43592 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWINDOW)
    Altura Manija = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Area = 2.44709616574625 (IFCAREAMEASURE) [SQUARE_METRE]
    DesfaseExterior = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    DesfaseInterior = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.0740311109803639 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Altura Real = 1480. (IFCLENGTHMEASURE) [MILLI METRE]
    Altura maxima = 2742. (IFCLENGTHMEASURE) [MILLI METRE]
    Altura minima = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    AnchoMarcoCentral = 141.4 (IFCLENGTHMEASURE) [MILLI METRE]
    AnchoMarcoPerimetral = 89.1 (IFCLENGTHMEASURE) [MILLI METRE]
    AnchoPoliamidaHoja = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    AnchoPoliamidaMarco = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Anchura Maxima = 1700. (IFCLENGTHMEASURE) [MILLI METRE]
    Anchura Minima = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Anchura Real = 1230. (IFCLENGTHMEASURE) [MILLI METRE]
    EspesorPerfilesAluminio = 1.5 (IFCLENGTHMEASURE) [MILLI METRE]
    GrosorAcristalamiento = 24. (IFCLENGTHMEASURE) [MILLI METRE]
    GrosorAcristalamiento Real = 24. (IFCLENGTHMEASURE) [MILLI METRE]
    GrosorHoja = 67. (IFCLENGTHMEASURE) [MILLI METRE]
    GrosorMarco = 60. (IFCLENGTHMEASURE) [MILLI METRE]
    GrosorMaximoAcristalamiento = 46. (IFCLENGTHMEASURE) [MILLI METRE]
    GrosorMinimoAcristalamiento = 12. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 1480. (IFCLENGTHMEASURE) [MILLI METRE]
    Perimetro = 5420. (IFCREAL)
    Peso = 0. (IFCREAL)
    Profundidad = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 1230. (IFCLENGTHMEASURE) [MILLI METRE]
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "## Street City, State Zip" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: Generic - 200mm" (IFCLABEL)
    Family and Type = "Basic Wall: Generic - 200mm" (IFCLABEL)
    Type = "Basic Wall: Generic - 200mm" (IFCLABEL)
    Type Id = "Basic Wall: Generic - 200mm" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWINDOW)
    Category = "Windows" (IFCLABEL)
    DetallePerfileria = TRUE (IFCBOOLEAN)
    Family = "2019_ES_Ventana_QSystems_Q67+_2-Hojas: 1230x1480 mm - Practicable" (IFCLABEL)
    Family and Type = "2019_ES_Ventana_QSystems_Q67+_2-Hojas: 1230x1480 mm - Practicable" (IFCLABEL)
    Head Height = 2180. (IFCLENGTHMEASURE) [MILLI METRE]
    Host Id = "Basic Wall: Generic - 200mm" (IFCLABEL)
    RealAbatible = FALSE (IFCBOOLEAN)
    RealPracticable = TRUE (IFCBOOLEAN)
    Type = "2019_ES_Ventana_QSystems_Q67+_2-Hojas: 1230x1480 mm - Practicable" (IFCLABEL)
    Type Id = "2019_ES_Ventana_QSystems_Q67+_2-Hojas: 1230x1480 mm - Practicable" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Walls" (IFCLABEL)
    Family Name = "Basic Wall" (IFCTEXT)
  Other | properties | on 1 type object
    Category = "Windows" (IFCLABEL)
    Family Name = "2019_ES_Ventana_QSystems_Q67+_2-Hojas" (IFCTEXT)
    InstruccionesEspeciales = "" (IFCTEXT)
    MaterialContenedor = "" (IFCTEXT)
    MaterialEnvase = "" (IFCTEXT)
    TipoEmbalajeProteccion = "" (IFCTEXT)
  Phasing | properties | on 2 objects (1 IFCWALLSTANDARDCASE, 1 IFCWINDOW)
    Phase Created = "New Construction" (IFCLABEL)
  Phasing | properties | on 1 type object
    Fecha Colocacion = "" (IFCTEXT)
    Fecha Suministro = "" (IFCTEXT)
    Responsable Compra = "" (IFCTEXT)
  Structural | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
    Structural Usage = "Non-bearing" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Basic Wall:Generic - 200mm" (IFCIDENTIFIER)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "2019_ES_Ventana_QSystems_Q67+_2-Hojas:1230x1480 mm - Practicable" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCWINDOW)
    Manufacturer = "QSystems" (IFCLABEL)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCWINDOW)
    Mark = "6" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "Generic - 200mm" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Autor = "Bimetica Parametric Design Services, S.L." (IFCTEXT)
    AñoProduccion = "" (IFCTEXT)
    BIMsupport = "https://bimsupport.info/es/fabricantes/alueuropa-q-systems-bim/" (IFCTEXT)
    Base Precio Producto 01 = "" (IFCTEXT)
    Base Precio Producto 02 = "" (IFCTEXT)
    Base Precio Producto 03 = "" (IFCTEXT)
    COBieCategoria = "IfcWindow" (IFCTEXT)
    Catálogo (URL) = "https://qsystemsaluminio.com//wp-content/uploads/2021/05/Q67-1.pdf" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Codigo = "" (IFCTEXT)
    CodigoBarras = "" (IFCTEXT)
    Condiciones de Venta = "" (IFCTEXT)
    CondicionesGeneralesDeContratacion = "" (IFCTEXT)
    ContenidoGarantia = "" (IFCTEXT)
    Description = "Ventana 2 Hojas Practicables Q67+ de QSystems" (IFCTEXT)
    DuracionVidaUtil = "" (IFCTEXT)
    EmailContacto = "info@qsystemsaluminio.com" (IFCTEXT)
    Ensayos y certificados (URL) = "" (IFCTEXT)
    EtiquetaModelo = "" (IFCTEXT)
    Exclusiones = "" (IFCTEXT)
    FechaCompra = "" (IFCTEXT)
    FechaEmisionElementoBIM = "03/12/2021" (IFCTEXT)
    FechaFinGarantia = "" (IFCTEXT)
    FechaInicioGarantia = "" (IFCTEXT)
    FechaVencimientoElementoBIM = "03/12/2022" (IFCTEXT)
    GarantiaExtendida = "" (IFCTEXT)
    Historial = "(RVT2019) Actualziación a estándar GDO-BIM y datos. (RVT2015) Creación del Elemento." (IFCTEXT)
    IdentificadorGarantia = "" (IFCTEXT)
    InformacionTecnica = "https://qsystemsaluminio.com//wp-content/uploads/2021/05/Q67_ficha-tecnica-1.pdf" (IFCTEXT)
    LugarEnsamblaje = "" (IFCTEXT)
    Manufacturer = "QSystems" (IFCTEXT)
    Marcado CE = FALSE (IFCBOOLEAN)
    MasterformatCodigo = "08 50 00" (IFCTEXT)
    MasterformatTitulo = "Windows" (IFCTEXT)
    Model = "Ventana Q67+ - 2 Hojas Practicable" (IFCTEXT)
    Numero de Declaracion de Prestaciones = "" (IFCTEXT)
    Numero de Licencia = "XXX-XXXX9536" (IFCTEXT)
    NumeroArticulo = "" (IFCTEXT)
    NumeroArticuloGlobalComercial = "" (IFCTEXT)
    NumeroSerie = "" (IFCTEXT)
    OmniClass Number = "23.30.20.00" (IFCTEXT)
    OmniClass Title = "Windows" (IFCTEXT)
    OmniclassCodigo = "23-17 13 00" (IFCTEXT)
    OmniclassTitulo = "Windows" (IFCTEXT)
    Pais de Venta = "" (IFCTEXT)
    Partida URL = "" (IFCTEXT)
    PeriodoGarantia = "" (IFCTEXT)
    PesoMáximoDeLaHoja = 0. (IFCREAL)
    Plataforma descaga contenido BIM = "www.bimetica.com" (IFCTEXT)
    PuntoDeContacto = "QSystems" (IFCTEXT)
    Referencia = "Q67+" (IFCTEXT)
    Referencia Contacto Comercial Venta = "QSystems" (IFCTEXT)
    ReferenciaContacto = "QSystems" (IFCTEXT)
    ReferenciaLote = "" (IFCTEXT)
    ResistenciaFuego = "" (IFCTEXT)
    Serie = "Q67+" (IFCTEXT)
    TelefonoContacto = "+34 91 895 58 00" (IFCTEXT)
    TiempoMedioEntreFallos = "" (IFCTEXT)
    Titular = "Alueuropa S.A." (IFCTEXT)
    Type Comments = "" (IFCTEXT)
    Type Mark = "47" (IFCTEXT)
    Type Name = "1230x1480 mm - Practicable" (IFCTEXT)
    UNSPSCCodigo = "30171600" (IFCTEXT)
    UNSPSCTitulo = "Windows" (IFCTEXT)
    URL = "http://qsystemsaluminio.com/" (IFCTEXT)
    URL Perfil BIM = "https://bimetica.com/es/objeto-bim-ventana-q-systems-q67+-2-hojas-2597.html" (IFCTEXT)
    URL Poliamida - Catálogo = "http://www.technoform.com/fileadmin/Technoform_Bautec/standardprofiles.html" (IFCTEXT)
    URL Poliamida = "http://www.technoform.es/" (IFCTEXT)
    URL de Declaracion de Prestaciones = "" (IFCTEXT)
    URLProducto = "https://qsystemsaluminio.com/q67-plus/" (IFCTEXT)
    Uniclass2.0Codigo = "Ss_15_50_25" (IFCTEXT)
    Uniclass2.0Titulo = "Doors, Windows And Glazing Survey Systems" (IFCTEXT)
    Version = "RVT2019" (IFCTEXT)
    Version Estandar GDO-BIM = "GDO-BIM V02" (IFCTEXT)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Center" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.7 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
  Analytical Properties | properties | on 1 type object
    Analytic Construction = "<None>" (IFCTEXT)
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "None" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Abatible = FALSE (IFCBOOLEAN)
    Altura de antepecho por defecto = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    CerramientoExterior = TRUE (IFCBOOLEAN)
    ConfiguracionPoliamidas = "277400 - 493600 - 964200" (IFCTEXT)
    ControlHumos = FALSE (IFCBOOLEAN)
    Estado = "" (IFCTEXT)
    Motorizada = FALSE (IFCBOOLEAN)
    NivelSeguridad = "" (IFCTEXT)
    Oscilobatiente = FALSE (IFCBOOLEAN)
    Practicable = TRUE (IFCBOOLEAN)
    RepisaExterior = TRUE (IFCBOOLEAN)
    RepisaInterior = TRUE (IFCBOOLEAN)
    SalidaEmergencia = FALSE (IFCBOOLEAN)
    Wall Closure = "By host" (IFCIDENTIFIER)
  Graphics | properties | on 1 type object
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  2019_ES_Ventana_QSystems_Q67+_2-Hojas:1230x1480 mm - Practicable:361645 | predefined | on 1 type object
  Analysis Results | properties | on 1 type object
    FactorSolarModificado = 0. (IFCREAL)
    FactorSombra = 0. (IFCREAL)
    Total Y𝑔 = 0.11 (IFCREAL)
    Total 𝐴𝑓 = 0.63524128 (IFCREAL)
    Total 𝐴𝑔 = 1.18515872 (IFCREAL)
    Total 𝑈𝑓 = 2.5 (IFCREAL)
    Total 𝑈𝑔 = 1.5 (IFCREAL)
    Total 𝑙𝑔 = 7.028 (IFCREAL)
    Y𝑔 P1 = 0.11 (IFCREAL)
    Y𝑔 P2 = 0.11 (IFCREAL)
    𝐴𝑓 P1 = 0.45116676 (IFCAREAMEASURE) [SQUARE_METRE]
    𝐴𝑓 P2 = 0.18407452 (IFCAREAMEASURE) [SQUARE_METRE]
    𝐴𝑔 V1 = 0.59257936 (IFCAREAMEASURE) [SQUARE_METRE]
    𝐴𝑔 V2 = 0.59257936 (IFCAREAMEASURE) [SQUARE_METRE]
    𝑈𝑓 P1 = 2.5 (IFCREAL)
    𝑈𝑓 P2 = 2.5 (IFCREAL)
    𝑈𝑔 V1 = 1.5 (IFCREAL)
    𝑈𝑔 V2 = 1.5 (IFCREAL)
    𝑈𝑤 = 2.27363287189629 (IFCREAL)
    𝑙𝑔 P1 = 4.4244 (IFCREAL)
    𝑙𝑔 P2 = 2.6036 (IFCREAL)
  Data | properties | on 1 type object
    Area = 1.8204 (IFCAREAMEASURE) [SQUARE_METRE]
    Clasificacion acustica = "38 (-1,-4) dB" (IFCTEXT)
    Clasificacion de carga mecanica = "" (IFCTEXT)
    CondicionesEvaluacion = "" (IFCTEXT)
    DescripcionEvaluacion = "" (IFCTEXT)
    EstanqueidadAgua = "Clase E9000" (IFCTEXT)
    FechaEvaluacion = "" (IFCTEXT)
    Fraccion de area de acristalamiento = 0.651043023511316 (IFCREAL)
    Infiltracion = 0. (IFCREAL)
    PermeabilidadAlAire = "Clase 4" (IFCTEXT)
    ResistenciaAlViento = "Clase C5" (IFCTEXT)
    Transmitancia termica = 2.27363287189629 (IFCREAL)
  General | properties | on 1 type object
    CertificadoMantenimiento = "" (IFCTEXT)
    CondicionesMantenimiento = "" (IFCTEXT)
    Contacto = "QSystems" (IFCTEXT)
    CosteMantenimiento = 0. (IFCREAL)
    FechaInstalacion = "" (IFCTEXT)
    FrecuenciaMantenimiento = "" (IFCTEXT)
    NormativaMantenimiento = "" (IFCTEXT)
    TrabajoMantenimiento = "" (IFCTEXT)
    UnidadMantenimiento = "" (IFCTEXT)
    UnidadMedicion = "" (IFCTEXT)
  Green Building Properties | properties | on 1 type object
    AcidificacionAtmosferica = 0. (IFCREAL)
    AcidificacionAtmosfericaPorUnidad = 0. (IFCREAL)
    AguaConsumida = 0. (IFCREAL)
    AguaConsumidaPorUnidad = 0. (IFCREAL)
    CambioClimatico = 0. (IFCREAL)
    CambioClimaticoPorUnidad = 0. (IFCREAL)
    CosteEnergeticoKwh = 0. (IFCREAL)
    CosteEnergeticoMj = 0. (IFCREAL)
    Creditos BREEAM = "" (IFCTEXT)
    Creditos LEED = "" (IFCTEXT)
    Declaracion Ambiental de Producto URL = "" (IFCTEXT)
    DestruccionCapaOzonoEstratosferica = 0. (IFCREAL)
    DestruccionCapaOzonoEstratosfericaPorUnidad = 0. (IFCREAL)
    EmisionCO2 = 0. (IFCREAL)
    Energia consumida = 0. (IFCREAL)
    EnergiaNoRenovableConsumida = 0. (IFCREAL)
    EnergiaNoRenovableConsumidaPorUnidad = 0. (IFCREAL)
    EnergiaPrimariaTotalConsumida = 0. (IFCREAL)
    EnergiaPrimariaTotalConsumidaPorUnidad = 0. (IFCREAL)
    EnergiaRenovableConsumida = 0. (IFCREAL)
    EnergiaRenovableConsumidaPorUnidad = 0. (IFCREAL)
    Eutrofizacion = 0. (IFCREAL)
    EutrofizacionPorUnidad = 0. (IFCREAL)
    FaltaDeRecursos = 0. (IFCREAL)
    FaltaDeRecursosPorUnidad = 0. (IFCREAL)
    FaseCicloVida = "" (IFCTEXT)
    FormacionFotoquimicaOzono = 0. (IFCREAL)
    FormacionFotoquimicaOzonoPorUnidad = 0. (IFCREAL)
    Fuente Datos LCA = "" (IFCTEXT)
    Porcentaje materiales reciclados = 0. (IFCREAL)
    ReferenciaUnidadFuncional = "" (IFCTEXT)
    ResiduoInerte = 0. (IFCREAL)
    ResiduoInertePorUnidad = 0. (IFCREAL)
    ResiduoRadioactivo = 0. (IFCREAL)
    ResiduoRadioactivoPorUnidad = 0. (IFCREAL)
    ResiduosNoPeligrosos = 0. (IFCREAL)
    ResiduosNoPeligrososPorUnidad = 0. (IFCREAL)
    ResiduosPeligrosos = 0. (IFCREAL)
    ResiduosPeligrososPorUnidad = 0. (IFCREAL)
    Unidad = "" (IFCTEXT)
    VidaUtilEsperada = "" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    Acabado = "Anodizado, lacado y acabados" (IFCTEXT)
    Acristalamiento = "Cristal - Vidrio claro templado" (IFCLABEL)
    Espuma = "" (IFCTEXT)
    Intercalario = "Technoform Warm Edge" (IFCLABEL)
    Marco = "Aluminio Anodizado, lacado" (IFCLABEL)
    Poliamida = "Technoform polyamide" (IFCLABEL)
  Visibility | properties | on 1 type object
    Manija = TRUE (IFCBOOLEAN)